

**ADT7X3 update instruction**

1. Copy the update file to the root directory of the USB disk. The file has format “.mpcupdate” such as “MPC\_V2.0.0.1.mpcupdate”.


2. Plug the USB disk to the USB port at rear side of ADT7X3.




3. Click icon  at top right of the main page.




4. Select System Service .



5. Select Firmware Update .



6. Select Udisk Update.



7. After selecting the version required for the update, the system will automatically start the update process. During the process, the version information and the progress will be displayed; after completed, the upgrade results of each component will be displayed, and then it will automatically restart the unit.

Note：（√= update succeed，X= update failed，--- = no update performed）