Bots.Terminal

Directions for user

# Install

Double-click the installation package to install the software. Follow the installation wizard to complete the installation process.

# Start the software

Double-click the icon to start the software.



Figure 1-1 startScreen

Figure 1-2 shows the main screen after correct startup.




Figure 1-2 main sreen

Click Lower right corner of software EN or ZH to set the language, as shown in Figure 1-3 After selecting a language, the application program restarts to switch to the selected language.




Figure 1-3 change language

# Scan

Click the [Scan] button to find the devices to be upgraded. Of course, you need to connect the device to your computer first, and make sure the driver is installed and communicating properly.




Figure 3-1 start scanning

After clicking scan, the software starts to scan the device, and the progress bar is displayed in the lower left corner of the software. At this time, users can click the button to stop scanning, as shown in Figure 3-2.




Figure 3-2 scanning

After the scan is complete, the software displays the devices to be upgraded, as shown in the figure 3-3







Figure 3-3 scan is complete

# Upgrade







After the upgrade page is initialized, click the button [UpgardeFile] in the upper left to select the local upgrade package.




Click the icon  to select the local upgrade file. Then click the button [APPLY] to jump to the last screen.



After the UpgradeFile is loaded,click the button [Upgrade] to start upgrading.





The device upgrade is complete.

Note: Software cannot be closed during the upgrade.